AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MPO Plug & Play
Standard MPO Cassette Fiber Optic Panel
Description
1-72 fiber 1U 19" standard MPO cassette fiber optic panel
Cassette front options
12 or 24 LC/UPC or SC/UPC ports
Cassette back options
One or two 12-fiber MPO couplers
Fiber type compatibility
OM1, OM2, OM3, OM4 & OS2
Panel front
Up to three removable pre-loaded
cassettes
Panel access
Top and front slide rail
Back Cable Management
Removable tray with strain relief
Front Cable Management
Tray with rings for patch cord routing
and protection
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Steel, colored black
Front cover
None
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant materials
Port identification
Numbers
Ordering Information - Panel
Fiber
Cassette
Size
Description
Units
Packaging
P/N
Capacity
Capacity
mm
Standard Blank MPO Cassette Fiber Optic Panel
1U
72
3
44.5x483x501
1/Box
27M00NV072A-BK1U
Continued on page C.5.2.1a
C.5.2.1