AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 7A
S/FTP 100 Ohm Horizontal Outdoor DJ MB LAN Cables
Description
4 pair S/FTP outdoor double-jacketed cables with
aluminum moisture-barrier
Frequency range
1-1000 MHz
Conductor
22 AWG Solid bare copper
Insulation
PO
Color code
Modified ANSI/TIA-568-C.2 (Solid colors)
Longitudinal water
None
blocking
Individual pair shield
Aluminum foil
Overall shield
Tin-coated copper braid
Drain wire
None
Inner jacket
PVC or LS0H
Radial water blocking
200µ Aluminum moisture-barrier (MB)
Outer jacket
UV resistant MDPE for outdoor use
Outer jacket color
Black
Standard & EU Directives Conformance
• Category 7A cable according to IEC 61156-5
• 1000 MHz cable according to EN 50288-9-1
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max.
Short term bend radius
8xOD mm
Long term bend radius
4xOD mm
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
70 Ohm/Km max.
Capacitance
56 pF/m max. @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
78% nom.
Ordering Information
Inner
Inner
Outer
OD
Weight
Description
Jacket
OD
Jacket
Packaging
P/N
mm
Kg/Km
Type
mm
Type
4-Pair 22 AWG S/FTP CAT7A Outdoor DJ MB Cable Black
PVC
7.2
MB+PE
12.0
135
500m drum
11S7AMN004A-BK2K
4-Pair 22 AWG S/FTP CAT7A Outdoor DJ MB Cable Black
PVC
7.2
MB+PE
12.0
135
1000m drum
11S7AMN004A-BK2L
4-Pair 22 AWG S/FTP CAT7A Outdoor DJ MB Cable Black
LS0H
7.2
MB+PE
12.0
135
500m drum
11S7AMN004B-BK2K
4-Pair 22 AWG S/FTP CAT7A Outdoor DJ MB Cable Black
LS0H
7.2
MB+PE
12.0
135
1000m drum
11S7AMN004B-BK2L
E.2.16