AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 5e
F/UTP 100 Ohm Horizontal Outdoor DJ LAN Cables
Description
4 pair F/UTP outdoor double-jacketed cables
Frequency range
1-100 MHz
Conductor
24 AWG Solid bare copper
Insulation
PO
Color code
ANSI/TIA-568-C.2
Water blocking
None
Shield
Overall aluminum foil
Drain wire
Single tin-coated copper solid wire
Inner jacket
PVC or LS0H
Outer jacket - Option A
1.8 mm UV resistant PVC compound for
outdoor use
Outer jacket - Option B
1.0 mm UV resistant MDPE for outdoor use
Outer jacket color
Black
Standard & EU Directives Conformance
• Category 5e cable according to IEC 61156-5
• Category 5e cable according to ANSI/TIA-568-C.2
• 100MHz cable according to EN 50288-2-1
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max.
Dynamic bend radius
8xOD mm min
Static bend radius
4xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max.
Capacitance
56 pF/m max. @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
69% nom.
Ordering Information
Inner
Outer
OD
Weight
Description
Jacket
Jacket
Packaging
P/N
mm
Kg/Km
Type
Type
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
PVC
PVC
9.5
100
500m drum
11P5EBN004A-BK2K
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
PVC
PVC
9.5
100
1000m drum
11P5EBN004A-BK2L
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
PVC
PE
7.9
60
500m drum
11P5EEN004A-BK2K
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
PVC
PE
7.9
60
1000m drum
11P5EEN004A-BK2L
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
LS0H
PVC
9.5
100
500m drum
11P5EBN004B-BK2K
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
LS0H
PVC
9.5
100
1000m drum
11P5EBN004B-BK2L
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
LS0H
PE
7.9
60
500m drum
11P5EEN004B-BK2K
4-Pair 24 AWG F/UTP CAT5e Outdoor DJ Cable Black
LS0H
PE
7.9
60
1000m drum
11P5EEN004B-BK2L
E.2.2