AT&T Cabling Systems
Outdoorline
AT&T Outdoorline
Outdoor Single Loose-Tube Dielectric
Armored Double-Jacket Optical Fiber Cables
Description
2-12 fibers outdoor single loose-tube dielectric armored
double-jacket FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
Single PBT jell-filled loose tube
Strength elements
Served swellable glass yarn
Inner jacket material
PE
Dielectric armor
Swellable glass yarn
Outer jacket material
UV-resistant PE
Fibers color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
30xOD mm
Long term bend radius
15xOD mm
Operating temperature
-30 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Ordering Information
FF: Fiber Type
Max. Load N
Cable OD
Weight
Description
Short
Long
Packaging
P/N
mm
Kg/Km
Term
Term
2-Fiber FO Outdoor Dielectric Armored
10.0
75.0
1000
500
2000m Drum
24D FF AN002N-BK2N
Single Loose-Tube DJ Cable
4-Fiber FO Outdoor Dielectric Armored
10.0
75.0
1000
500
2000m Drum
24D FF AN004N-BK2N
Single Loose-Tube DJ Cable
6-Fiber FO Outdoor Dielectric Armored
10.0
75.0
1000
500
2000m Drum
24D FF AN006N-BK2N
Single Loose-Tube DJ Cable
8-Fiber FO Outdoor Dielectric Armored
10.0
75.0
1000
500
2000m Drum
24D FF AN008N-BK2N
Single Loose-Tube DJ Cable
10-Fiber FO Outdoor Dielectric Armored
10.0
75.0
1000
500
2000m Drum
24D FF AN010N-BK2N
Single Loose-Tube DJ Cable
12-Fiber FO Outdoor Dielectric Armored
10.0
75.0
1000
500
2000m Drum
24D FF AN012N-BK2N
Single Loose-Tube DJ Cable
E.4.4