AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor/Outdoor Multi Loose-Tube Dry-Core Single Jacket Optical Fiber LS0H Cables
Description
2-288 fibers indoor/outdoor all-dielectric multi loose-tube dry-core
single-jacket non-armored FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
PBT jell-filled loose tubes
Central strength member
Rigid all-dielectric FRP
Water blocking elements
Swellable yarn and tapes
Cable jacket material
Flame retardant LS0H UV-resistant
compound
Fibers and tubes color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-40 to +70C
Installation temperature
0 to +50C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Default fiber count per tube
Indicated (other options available)
Ordering Information
FF: Fiber Type
Fibers
Cable
Max. Load N
Tube
Weight
Description
per
Fillers
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Tube
mm
Term
Term
2-Fiber Indoor/Outdoor LS0H FO
2000m
2
1
5
10.0
95
1500
900
25R FF HA002N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
4-Fiber Indoor/Outdoor LS0H FO
2000m
4
1
5
10.0
95
1500
900
25R FF HA004N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
6-Fiber Indoor/Outdoor LS0H FO
2000m
6
1
5
10.0
95
1500
900
25R FF HA006N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
8-Fiber Indoor/Outdoor LS0H FO
2000m
4
2
4
10.0
95
1500
900
25R FF HA008N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
12-Fiber Indoor/Outdoor LS0H FO
2000m
4
3
3
10.0
95
1500
900
25R FF HA012N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
24-Fiber Indoor/Outdoor LS0H FO
2000m
6
4
2
10.0
96
1500
900
25R FF HA024N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
36-Fiber Indoor/Outdoor LS0H FO
2000m
6
6
0
11.0
116
1500
900
25R FF HA016N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
48-Fiber Indoor/Outdoor LS0H FO
2000m
8
6
0
11.0
117
1500
900
25R FF HA048N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
72-Fiber Indoor/Outdoor LS0H FO
2000m
12
6
0
11.5
130
1500
900
25R FF HA072N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
96-Fiber Indoor/Outdoor LS0H FO
2000m
12
8
0
13.5
165
1500
900
25R FF HA096N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
144-Fiber Indoor/Outdoor LS0H FO
2000m
12
12
0
17.0
250
1500
900
25R FF HA144N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
288-Fiber Indoor/Outdoor LS0H FO
2000m
12
24
0
19.5
320
1500
900
25R FF HA288N-BK2N
Loose-Tube All-Dielectric Dry-Core SJ Cable
Drum
B.1.2.3