AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 3
U/UTP 100 Ohm Horizontal and Backbone Outdoor DJ MB LAN Cables
Description
4-900 pair U/UTP outdoor double-jacketed cables with aluminum
moisture-barrier
Frequency range
1-16 MHz
Conductor
24 AWG Solid bare copper
Insulation
PO
Longitudinal water blocking
Petroleum jelly
Color code
Modified ANSI/ICEA S-80-576
Shield
None
Inner jacket
Heavy duty UV resistant PE
Radial water blocking
200µ Aluminum moisture-barrier (MB)
Outer jacket
UV resistant MDPE for outdoor use
Jacket color
Black
Standard & EU Directives Conformance
• Category 3 cable according to IEC 61156-4
• Category 3 cable according to ANSI/TIA-568-C.2
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max
Dynamic bend radius
50xOD mm min
Static bend radius
25xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max
Capacitance
66 pF/m max. @ 1KHz
Voltage rating
75 Vdc max
Velocity of propagation (NVP)
69% nom.
Ordering Information
Inner OD
Jacket
OD
Weight
Description
Packaging
P/N
mm
Type
mm
Kg/Km
4-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
7.2
MB+PE
11.9
63
500m Drum
11U03MN004N-BK2K
4-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
7.2
MB+PE
11.9
63
1000m Drum
11U03MN004N-BK2L
25-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
12
MB+PE
16.7
236
1000m Drum
11U03MN025N-BK2L
100-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
21
MB+PE
25.4
738
1000m Drum
11U03MN100N-BK2L
200-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
28
MB+PE
33
1520
500m Drum
11U03MN200N-BK2K
300-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
34
MB+PE
39
2170
500m Drum
11U03MN300N-BK2K
400-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
38
MB+PE
43
2750
500m Drum
11U03MN400N-BK2K
600-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
47
MB+PE
52
4050
500m Drum
11U03MN600N-BK2K
900-Pair 24 AWG U/UTP CAT3 Outdoor DJ MB Cable Black
56
MB+PE
61
5835
500m Drum
11U03MN900N-BK2K
E.1.2