AT&T Cabling Systems
FiberLine
AT&T FiberLine
Outdoor Tight-Buffer Steel Armored
Double-Jacket Optical Fiber Cables
Description
2-144 fibers indoor/outdoor tight-buffer steel armored
double-jacket FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
900µ tight flame retardant LS0H
coating
Strength elements
Served swellable aramid and glass
yarn
Sub-units jacket material
Flame retardant LS0H compound
Multi-unit water blocking
Swellable tapes
Inner jacket material
Flame retardant LS0H compound
Armor
Corrugated steel tape
Water blocking
Petroleum jelly
Outer jacket material
UV-resistant PE
Fibers and sub-units color code TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-30 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Ordering Information - Single Unit Cables
FF: Fiber Type
Cable
Max. Load N
Fiber
Weight
Description
OD
Packaging
P/N
Short
Long
Count
Kg/Km
mm
Term
Term
2-Fiber FO Outdoor Steel Armored
2
8.5
90
1000
400
2000m Drum
23D FF CN002S-BK2N
Tight-Buffer DJ Cable
4-Fiber FO Outdoor Steel Armored
4
10.0
110
1000
400
2000m Drum
23D FF CN004S-BK2N
Tight-Buffer DJ Cable
6-Fiber FO Outdoor Steel Armored
6
10.0
110
1000
400
2000m Drum
23D FF CN006S-BK2N
Tight-Buffer DJ Cable
8-Fiber FO Outdoor Steel Armored
8
10.5
125
1000
400
2000m Drum
23D FF CN008S-BK2N
Tight-Buffer DJ Cable
12-Fiber FO Outdoor Steel Armored
12
11.5
140
1000
400
2000m Drum
23D FF CN012S-BK2N
Tight-Buffer DJ Cable
16-Fiber FO Outdoor Steel Armored
16
12.0
155
1700
800
2000m Drum
23D FF CN016S-BK2N
Tight-Buffer DJ Cable
18-Fiber FO Outdoor Steel Armored
18
12.5
165
1700
800
2000m Drum
23D FF CN018S-BK2N
Tight-Buffer DJ Cable
24-Fiber FO Outdoor Steel Armored
24
13.5
185
1700
800
2000m Drum
23D FF CN024S-BK2N
Tight-Buffer DJ Cable
Continued on page B.1.7.7a
B.1.7.7