AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 3
F/UTP 100 Ohm Horizontal and Backbone Outdoor SJ LAN Cables
Description
4-900 pair F/UTP shielded cables
Frequency range
1-16 MHz
Conductor
24 AWG Solid bare copper
Insulation
PO
Water blocking
Petroleum jelly
Color code
Modified ANSI/ICEA S-80-576
Shield
Overall aluminum foil
Drain wire
Solid tin-coated copper wire
Jacket
Heavy duty UV resistant PE
Jacket color
Black
Standard & EU Directives Conformance
• Category 3 cable according to IEC 61156-4
• Category 3 cable according to ANSI/TIA-568-C.2
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max
Dynamic bend radius
8xOD mm min
Static bend radius
4xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max
Capacitance
66 pF/m max. @ 1KHz
Voltage rating
75 Vdc max
Velocity of propagation (NVP)
69% nom.
Ordering Information
OD
Weight
Description
Packaging
P/N
mm
Kg/Km
4-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
7.2
45
500m Drum
11P03EN004N-BK2K
4-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
7.2
45
1000m Drum
11P03EN004N-BK2L
25-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
14.0
210
1000m Drum
11P03EN025N-BK2L
100-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
24.5
910
1000m Drum
11P03EN100N-BK2L
200-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
33
1250
500m Drum
11P03EN200N-BK2K
300-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
38
1850
500m Drum
11P03EN300N-BK2K
400-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
45
2400
500m Drum
11P03EN400N-BK2K
600-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
55
3570
500m Drum
11P03EN600N-BK2K
900-Pair 24 AWG F/UTP CAT3 Outdoor SJ Cable Black
65
5400
500m Drum
11P03EN900N-BK2K
E.1.4