AT&T Cabling Systems
RackLine
AT&T RackLine
Free Standing Server Cabinets
Description
Free standing 19” server cabinets
Construction material
Sheet Steel
Size options
26U, 42U and 47U
(other sizes available)
Width and depth options
600x1000mm or 800x1000mm
Color
Black RAL 9005
Accessories
Page D.5.1
Standard & EU Directives Conformance
• Mechanical structure conforming to EN 61587-1,
IEC 60917 & IEC 60297
• Vibration & shock tests according to IEC 60068-2
• Corrosion resistance (salt spray) acc. to ISO 9227, ASTM B117
• IP20 according to IEC 60529
• Bonding & ground continuity according to IEC 61010-1
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Static load capacity
1000 Kg max.
Dynamic load capacity
750 Kg max.
Front door
Detachable, single, 82% perforated
Rear door
Detachable, double, 82% perforated
Side panels
Detachable, key-locked
Profiles
U marking on both sides
Mounting
Normal floor or raised floor
Optional raised floor fixing kit
Electrical grounding
Internal parts and frame grounding kit
Cabinet row formation
Aligning baying kit
Locking options
Standard: Mechanical lock
Optional: Electronic key-access
Ordering Information
Dimensions
Description
Size
Color
P/N
mm
Free standing 19" Server Cabinet
26U
600x1000
Black
7116100026A-BK51
Free standing 19" Server Cabinet
42U
600x1000
Black
7116100042A-BK51
Free standing 19" Server Cabinet
47U
600x1000
Black
7116100047A-BK51
Free standing 19" Server Cabinet
42U
800x1000
Black
7118100042A-BK51
Free standing 19" Server Cabinet
47U
800x1000
Black
7118100047A-BK51
Free standing 19" Server Cabinet
26U
600x1000
Gray
7116100026A-GY51
Free standing 19" Server Cabinet
42U
600x1000
Gray
7116100042A-GY51
Free standing 19" Server Cabinet
47U
600x1000
Gray
7116100047A-GY51
Free standing 19" Server Cabinet
42U
800x1000
Gray
7118100042A-GY51
Free standing 19" Server Cabinet
47U
800x1000
Gray
7118100047A-GY51
D.1