AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 3
U/UTP 100 Ohm Horizontal and Backbone Outdoor DJ CSA LAN Cables
Description
4-900 pair U/UTP outdoor double-jacketed cables with
corrugated steel tape armor
Frequency range
1-16 MHz
Conductor
24 AWG Solid bare copper
Insulation
PO
Longitudinal water blocking
Petroleum jelly
Color code
Modified ANSI/ICEA S-80-576
Shield
None
Inner jacket
Heavy duty UV resistant PE
Armor and radial water blocking
150µ Corrugated steel tape
armor (CSA)
Outer jacket
UV resistant MDPE for outdoor use
Jacket color
Black
Standard & EU Directives Conformance
• Category 3 cable according to IEC 61156-4
• Category 3 cable according to ANSI/TIA-568-C.2
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max
Dynamic bend radius
50xOD mm min
Static bend radius
25xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max
Capacitance
66 pF/m max. @ 1KHz
Voltage rating
75 Vdc max
Velocity of propagation (NVP)
69% nom.
Ordering Information
Inner OD
Jacket
OD
Weight
Description
Packaging
P/N
mm
Type
mm
Kg/Km
4-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
7.2
CSA+PE
12.8
96
500m Drum
11U03CN004N-BK2K
4-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
7.2
CSA+PE
12.8
96
1000m Drum
11U03CN004N-BK2L
25-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
12
CSA+PE
17.5
260
1000m Drum
11U03CN025N-BK2L
100-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
21
CSA+PE
26.5
775
1000m Drum
11U03CN100N-BK2L
200-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
28
CSA+PE
33.5
1585
500m Drum
11U03CN200N-BK2K
300-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
34
CSA+PE
40
2235
500m Drum
11U03CN300N-BK2K
400-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
38
CSA+PE
43
2825
500m Drum
11U03CN400N-BK2K
600-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
47
CSA+PE
52
4145
500m Drum
11U03CN600N-BK2K
900-Pair 24 AWG U/UTP CAT3 Outdoor DJ CSA Cable Black
56
CSA+PE
62
5945
500m Drum
11U03CN900N-BK2K
E.1.3