AT&T Cabling Systems
CenterLine
AT&T CenterLine
DC LCD Rack Consoles
Description
1U LCD consoles with optional KVM module for quick server access
LCD display
17"
Mounting
Rack mount - 1U
Connectivity options
Single or multi-port (KVM)
KVM options
8 or 16 ports
IP remote connectivity option
NIC with RJ45 port
Cable remote connectivity
Console Extender Module up to
option
150m
Supported interfaces
PS2 and USB
Supported platforms
DOS, Windows, Netware, Unix,
Linux and Mac OS
Standard & EU Directives Conformance
• EN 55022 Class B & EN 55024 (EMC)
• EN 61000-3-2 & EN 61000-3-3
• EN 60950-1 (Safety)
• EU 2006/95/EC (LVD)
• EU 2011/65/EU (RoHS-2)
• EU 89/336/EEC (EMC)
Features and Properties
Computer selection method
On screen display (OSD) or
hot-key push button
Server connections
1-128
Daisy chaining
Up to 8 levels
Auto scan intervals
5-99 seconds
Physically connected remote console
Up to 300m
IP-based remote module
10/100 Mbps Ethernet NIC
Keyboard & mouse emulation
PS/2
Video resolution - local console
1280x1024 pixels
Video resolution - remote console
Up to 1600x1200 pixels
Housing
Metal case
Ordering Information - LCD Consoles
Dimensions
Description
Size
Ports
Servers
P/N
mm
Rack Mount 17” LCD Console
1U
1
1
600x450x44
4311001001A-MT51
Rack Mount 17” LCD Console with KVM Switch
1U
8
64
600x450x44
4321008064A-MT51
Rack Mount 17” LCD Console with KVM Switch
1U
16
128
600x450x44
4321016128A-MT51
Ordering Information - Modules
Description
Port
Module Type
P/N
IP Module
RJ45
DIP-101
43300RJ45PM-NS51
Console Extender Module
RJ45
DCC100R/T
43300RJ45PM-NS51
Ordering Information - Cables
Cable Terminations
Cable Length
Description
P/N
Console Side
Server Side
m
PS/2 Combo KVM cable
1xVGA
2xPS/2
1xVGA
1.8
4340PS2018A-NS51
PS/2 Combo KVM cable
1xVGA
2xPS/2
1xVGA
3.0
4340PS2030A-NS51
PS/2 Combo KVM cable
1xVGA
2xPS/2
1xVGA
5.0
4340PS2050A-NS51
USB Combo KVM cable
1xVGA
1xUSB
1xVGA
1.8
4340USB018A-NS51
USB Combo KVM cable
1xVGA
1xUSB
1xVGA
3.0
4340USB030A-NS51
USB Combo KVM cable
1xVGA
1xUSB
1xVGA
5.0
4340USB050A-NS51
C.3