AT&T Cabling Systems
CopperLine
AT&T CopperLine Outlets
LJ6C (UK) Style Faceplates
Description
1-4 port LJ6C Style faceplates
Jack compatibility
Shielded or unshielded RJ45
keystone jacks
Category compatibility
CAT5e CAT6 CAT6A
Mount type
Wall or ducts
Shuttered
Yes
Color
White (other colors available)
KSJ insertion method
Back loading
Standard & EU Directives Conformance
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Material of construction
High-impact flame retardant
materials
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Storage temperature
-20 to +80C
Ordering Information
Size
Description
Color
Ports
Labeling
Packaging
P/N
mm
LJ6C Style Standard Shallow Back Box
White
N/A
87x87x28
None
1/Bag
16L00NV000A-WT61
LJ6C Style Standard Deep Back Box
White
N/A
87x87x42
None
1/Bag
16L00NV000B-WT61
LJ6C Style Wide Shallow Back Box
White
N/A
147x87x28
None
1/Bag
16L00NV000C-WT61
LJ6C Style Wide Deep Back Box
White
N/A
147x87x42
None
1/Bag
16L00NV000D-WT61
LJ6C Style Standard Faceplate for A Single Module
White
N/A
86x86x9
None
1/Bag
16L00NV000E-WT61
LJ6C Style Standard Faceplate for Two Modules
White
N/A
86x86x9
None
1/Bag
16L00NV000F-WT61
LJ6C Style Wide Faceplate for Four Modules
White
N/A
146x86x9
None
1/Bag
16L00NV000G-WT61
LJ6C Style Flat Module
White
1
38x25
Station ID
1/Bag
16L00NV001A-WT61
LJ6C Style Angled Module
White
1
38x25
Station ID
1/Bag
16L00NV001B-WT61
LJ6C Style Blank Flat Module
White
0
38x25
None
1/Bag
16L00NV000H-WT61
A.11.3