AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor Breakout Optical Fiber LS0H Cables
Description
1-12 fibers indoor breakout FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
900µ tight flame retardant LS0H
coating
Strength elements
Served aramid and glass yarn
Minicable jacket material
Flame retardant LS0H compound
Minicable jacket diameter
2.0 mm nom. (other sizes available)
Color code
TIA-598-C
Jacket color
Per request
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
MM OM1 & OM2: Orange
MM OM3: Turquoise
Default jacket colors
MM OM4: Purple
SM: Yellow
Panel Ordering Information
FF: Fiber Type CC: Jacket Color
OD
Weight
Max. Load N
Description
Packaging
P/N
mm
Kg/Km
Short Term
Long Term
2-Fiber LS0H FO Indoor Breakout Cable
6.5
45
400
200
2000m Drum
22N FF HA002N-CC 2N
4-Fiber LS0H FO Indoor Breakout Cable
7.0
50
1000
500
2000m Drum
22N FF HA004N-CC 2N
6-Fiber LS0H FO Indoor Breakout Cable
8.3
65
1200
600
2000m Drum
22N FF HA006N-CC 2N
8-Fiber LS0H FO Indoor Breakout Cable
9.5
85
1400
600
2000m Drum
22N FF HA008N-CC 2N
12-Fiber LS0H FO Indoor Breakout Cable
12.5
150
1500
600
2000m Drum
22N FF HA012N-CC 2N
B.1.1.3