AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 3
Unshielded RJ45 Patch Panels
Description
25 or 50 port unshielded panels
Frequency range
1-16 MHz
Compatible conductors
23-26 AWG Solid or stranded
Wiring
2 pairs per port: 3-6 & 4-5
Blocks
IDC 110 or LSA-Plus
Shield
None
Housing
High impact FR compound
Frame
Galvanized steel
Standard & EU Directives Conformance
• Category 3 connecting hardware according to
ANSI/TIA-568-C.2
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Construction
5 modules of fixed 5-ports or
10-ports PCB units.
Port contacts
50µ-Inch gold plating
Insertion/Extraction durability
750 cycles Level A durability
Cable re-termination
20 terminations
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Contact resistance
20 mOhm max.
DC resistance
0.2 Ohm max.
Voltage rating
75 Vdc max.
Insulation resistance
10 MegaOhm min. @500 Vdc
Ordering Information
Size
Description
Color
Blocks
Units
Packaging
P/N
mm
25 Port RJ45 Unshielded CAT3 19’’ Patch Panel
Black
110 IDC
1U
44.4x483
1/Box
13U03NV025A-BK1U
25 Port RJ45 Unshielded CAT3 19’’ Patch Panel
Black
LSA-Plus
1U
44.4x483
1/Box
13U03NV025B-BK1U
50 Port RJ45 Unshielded CAT3 19’’ Patch Panel
Black
110 IDC
1U
44.4x483
1/Box
13U03NV050A-BK1U
50 Port RJ45 Unshielded CAT3 19’’ Patch Panel
Black
LSA-Plus
1U
44.4x483
1/Box
13U03NV050B-BK1U
<
A.1.3