AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 7
S/FTP 100 Ohm Horizontal Outdoor DJ CSA LAN Cables
Description
4 pair S/FTP outdoor double-jacketed cables with corrugated steel
tape armor
Frequency range
1-600 MHz
Conductor
23 AWG Solid bare copper
Insulation
PO
Color code
Modified ANSI/TIA-568-C.2 (Solid colors)
Longitudinal water
None
blocking
Individual pair shield
Aluminum foil
Overall shield
Tin-coated copper braid
Drain wire
None
Inner jacket
PVC or LS0H
Armor and radial water
150µ Corrugated steel tape armor (CSA)
blocking
Outer jacket
UV resistant MDPE for outdoor use
Outer jacket color
Black
Standard & EU Directives Conformance
• Category 7 cable according to IEC 61156-5
• 600 MHz cable according to EN 50288-4-1
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max.
Dynamic bend radius
50xOD mm min
Static bend radius
25xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
80 Ohm/Km max.
Capacitance
56 pF/m max. @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
78% nom.
Ordering Information
Inner
Inner
Outer
OD
Weight
Description
Jacket
OD
Jacket
Packaging
P/N
mm
Kg/Km
Type
mm
Type
4-Pair 23 AWG S/FTP CAT7 Outdoor DJ CSA Cable Black
PVC
7.0
CSA+PE
12.7
150
500m drum
11S07CN004A-BK2K
4-Pair 23 AWG S/FTP CAT7 Outdoor DJ CSA Cable Black
PVC
7.0
CSA+PE
12.7
150
1000m drum
11S07CN004A-BK2L
4-Pair 23 AWG S/FTP CAT7 Outdoor DJ CSA Cable Black
LS0H
7.0
CSA+PE
12.7
150
500m drum
11S07CN004B-BK2K
4-Pair 23 AWG S/FTP CAT7 Outdoor DJ CSA Cable Black
LS0H
7.0
CSA+PE
12.7
150
1000m drum
11S07CN004B-BK2L
E.2.14