AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor Simplex and Duplex Optical Fiber LS0H Cables
Description
1-2 fibers indoor simplex and duplex FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
900µ tight flame retardant LS0H
coating
Strength elements
Served aramid and glass yarn
Minicable jacket material
Flame retardant LS0H compound
Color code
1. Blue 2. Orange
Jacket color
Per request
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
MM OM1 & OM2: Orange
MM OM3: Turquoise
Default jacket colors
MM OM4: Purple
SM: Yellow
Panel Ordering Information
FF: Fiber Type CC: Jacket Color
OD
Weight
Max. Load N
Description
Packaging
P/N
mm
Kg/Km
Short Term
Long Term
Simplex LS0H FO Indoor Cable
1.8
3.5
80
40
2000m Drum
21N FF HA001A-CC 2N
Simplex LS0H FO Indoor Cable
2.0
3.9
100
50
2000m Drum
21N FF HA001B-CC 2N
Simplex LS0H FO Indoor Cable
2.4
4.5
100
50
2000m Drum
21N FF HA001C-CC 2N
Simplex LS0H FO Indoor Cable
2.8
5.2
120
60
2000m Drum
21N FF HA001D-CC 2N
Simplex LS0H FO Indoor Cable
3.0
6.5
160
80
2000m Drum
21N FF HA001E-CC 2N
Duplex LS0H FO Indoor Zip-Cable
1.8x3.6
7.0
160
80
2000m Drum
21N FF HA001A-CC 2N
Duplex LS0H FO Indoor Zip-Cable
2.0x4.0
8.0
200
100
2000m Drum
21N FF HA001B-CC 2N
Duplex LS0H FO Indoor Zip-Cable
2.4x4.8
9.1
240
120
2000m Drum
21N FF HA001C-CC 2N
Duplex LS0H FO Indoor Zip-Cable
2.8x5.6
10.5
300
150
2000m Drum
21N FF HA001D-CC 2N
Duplex LS0H FO Indoor Zip-Cable
3.0x6.0
14.0
300
150
2000m Drum
21N FF HA001E-CC 2N
B.1.1.1