AT&T Cabling Systems
CopperLine
AT&T CopperLine Panels
Shielded Snap-in Blank High-Density Patch Panels
Description
48 port shielded high-density blank 19” panels
KSJ type compatibility
Shielded or unshielded
180° straight RJ45 jacks
Category compatibility
CAT5e CAT6 CAT6A
KSJ insertion method
Back loading
Formation
48 ports in two rows (1U)
Front cable organizer
None
Back cable organizer
Rigid frame
Shield
All shielded jacks grounded
through the panel
Standard & EU Directives Conformance
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Galvanized corrosion resistant
steel
Paint
Powder paint finish
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Storage temperature
-20 to +80C
Plastic parts
High-impact flame retardant
materials
Port identification
Printed numbers (1-48)
Panel identification
Designated space at the panel
front
Ordering Information
Size
Description
Color
Units
Packaging
P/N
mm
48 Port Shielded 19’’ Snap-in Blank High Density Patch Panel
Metal
1U
44.4x483
1/Box
13S00NV048C-MT1U
A.10.2.3