AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic FC/UPC Simplex Singlemode Cords
Description
This page shows some of the available combinations of AT&T fiber-optic
Simplex Singlemode Cords made with singlemode fibers and terminated
with FC/UPC connectors.
Additional combinations can be selected using the information on page B.3
Fiber type
Select a singlemode fiber from page B.6
Buffer type
900µ tight flame retardant LS0H coating
Strength elements
Served aramid and glass yarn
Minicable jacket material
Flame retardant LS0H compound
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
Default jacket color
Yellow
Ordering Information
FF: Fiber Type
Length
Cable OD
Description
Packaging
P/N
m
mm
FC/UPC-FC/UPC Simplex Singlemode Cord LS0H
1
3.0
1/Bag - 12/Box
28C FF FF010T-YL61
FC/UPC-FC/UPC Simplex Singlemode Cord LS0H
2
3.0
1/Bag - 12/Box
28C FF FF020T-YL61
FC/UPC-FC/UPC Simplex Singlemode Cord LS0H
3
3.0
1/Bag - 12/Box
28C FF FF030T-YL61
FC/UPC-FC/UPC Simplex Singlemode Cord LS0H
5
3.0
1/Bag - 12/Box
28C FF FF050T-YL61
FC/UPC-FC/UPC Simplex Singlemode Cord LS0H
10
3.0
1/Bag - 12/Box
28C FF FF100T-YL61
FC/UPC-ST/UPC Simplex Singlemode Cord LS0H
1
3.0
1/Bag - 12/Box
28C FF FC010T-YL61
FC/UPC-ST/UPC Simplex Singlemode Cord LS0H
2
3.0
1/Bag - 12/Box
28C FF FC020T-YL61
FC/UPC-ST/UPC Simplex Singlemode Cord LS0H
3
3.0
1/Bag - 12/Box
28C FF FC030T-YL61
FC/UPC-ST/UPC Simplex Singlemode Cord LS0H
5
3.0
1/Bag - 12/Box
28C FF FC050T-YL61
FC/UPC-ST/UPC Simplex Singlemode Cord LS0H
10
3.0
1/Bag - 12/Box
28C FF FC100T-YL61
FC/UPC-FC/APC Simplex Singlemode Cord LS0H
1
3.0
1/Bag - 12/Box
28C FF FG010T-YL61
FC/UPC-FC/APC Simplex Singlemode Cord LS0H
2
3.0
1/Bag - 12/Box
28C FF FG020T-YL61
FC/UPC-FC/APC Simplex Singlemode Cord LS0H
3
3.0
1/Bag - 12/Box
28C FF FG030T-YL61
FC/UPC-FC/APC Simplex Singlemode Cord LS0H
5
3.0
1/Bag - 12/Box
28C FF FG050T-YL61
FC/UPC-FC/APC Simplex Singlemode Cord LS0H
10
3.0
1/Bag - 12/Box
28C FF FG100T-YL61
FC/UPC-LC/APC Simplex Singlemode Cord LS0H
1
2.0
1/Bag - 12/Box
28C FF FR010T-YL61
FC/UPC-LC/APC Simplex Singlemode Cord LS0H
2
2.0
1/Bag - 12/Box
28C FF FR020T-YL61
FC/UPC-LC/APC Simplex Singlemode Cord LS0H
3
2.0
1/Bag - 12/Box
28C FF FR030T-YL61
FC/UPC-LC/APC Simplex Singlemode Cord LS0H
5
2.0
1/Bag - 12/Box
28C FF FR050T-YL61
FC/UPC-LC/APC Simplex Singlemode Cord LS0H
10
2.0
1/Bag - 12/Box
28C FF FR100T-YL61
FC/UPC-LSH/UPC Simplex Singlemode Cord LS0H
1
2.0
1/Bag - 12/Box
28C FF FL010T-YL61
FC/UPC-LSH/UPC Simplex Singlemode Cord LS0H
2
2.0
1/Bag - 12/Box
28C FF FL020T-YL61
FC/UPC-LSH/UPC Simplex Singlemode Cord LS0H
3
2.0
1/Bag - 12/Box
28C FF FL030T-YL61
FC/UPC-LSH/UPC Simplex Singlemode Cord LS0H
5
2.0
1/Bag - 12/Box
28C FF FL050T-YL61
FC/UPC-LSH/UPC Simplex Singlemode Cord LS0H
10
2.0
1/Bag - 12/Box
28C FF FL100T-YL61
Examples
FC/UPC-FC/UPC Simplex Singlemode Cord LS0H OS2 Yellow
1
3.0
1/Bag - 12/Box
28CS2FF010T-YL61
FC/UPC-FC/APC Simplex Singlemode Cord LS0H G.652.D Yellow
5
3.0
1/Bag - 12/Box
28CM3FG050T-YL61
FC/UPC-LSH/UPC Simplex Singlemode Cord LS0H G.657.A2 Yellow
10
2.0
1/Bag - 12/Box
28CA2FL100T-YL61
B.3.1.3.2