AT&T Cabling Systems
FiberLine
AT&T FiberLine Panels
High-Density 19” Fiber Optic Panel
Description
1-72 fiber 1U high-density 19" fiber optic splicing/distribution panel
Connector type compatibility - Group A ST, SC, FC
Connector type compatibility - Group B LC, MTRJ, LSH (E-2000™)
Splicing with Group A connectors
Up to three 12 fiber
splicing cassettes
Splicing with Group B connectors
Up to three 24 fiber
splicing cassettes
Distribution with Group A connectors
Up to 36 fiber direct cable
termination
Distribution with Group B connectors
Up to 72 fiber direct cable
termination
Panel front
Up to three removable
pre-loaded modules
Panel access
Top and front slide rail
Back Cable Management
Tray Side & back cable
entry with strain relief
Front Cable Management
Tray with rings for patch
cord routing and protection
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
SPCC Steel, colored black
Front cover
None
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant materials
Port identification
Numbers and designated space
printed on the cover
Ordering Information - Panel
Fiber
Cassette
Module
Size
Description
Units
Capacity
Packaging
P/N
Capacity
Capacity
mm
A
B
High-Density Blank 19” Fiber Optic Panel
1U
36
72
3
3
44.5x483x501
1/Box
27H00NV072A-BK1U
Continued on page B.2.1.2a
B.2.1.2