AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic ST Connectors and Couplers
Description
Fiber Optic Connectors and Couplers Type ST
Durability
0.2dB max. change after 1000 mating cycles
Temperature range
-20 to +60C
Typical Insertion loss
<0.2dB
Connector Ferrule type Ceramic
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• EU Directive 2011/65/EU (RoHS-2)
Notes:
a. Each product has a full-length P/N that can be used as ordering information.
b. Each connector has a single letter code that can be used to build fiber-optic cords and pigtails part-numbers.
c. The default colors are indicated in this page. Other options available.
d. Each bag contains one connector and two colored boots: 0.9mm & 3.0mm.
Ordering Information - Connectors
Compatible
Body
Type
Formation
Boot Color
Code
Packaging
P/N
Fiber
Color
ST/UPC Connector
Multimode
Single
Metal
Black
A
1/Bag 120/Box
29CM1NV001A-BK61
ST/UPC Connector
Multimode
Single
Metal
Red
A
1/Bag 120/Box
29CM1NV001A-RD61
ST/UPC Connector
Singlemode
Single
Metal
Yellow
C
1/Bag 120/Box
29CS1NV001C-YL61
Ordering Information - Couplers
Compatible
Body
Cover
Type
Formation
Sleeve
Packaging
P/N
Fiber
Color
Color
ST/UPC Coupler
Multimode
Single
Metal
Black
PB
1/Bag 120/Box
29LM1NV001A-BK61
ST/UPC Coupler
Singlemode
Single
Metal
Yellow
Zirconia
1/Bag 120/Box
29LS1NV001C-YL61
B.4.1.1