AT&T Cabling Systems
FiberLine
AT&T FiberLine
Outdoor Tight-Buffer Steel Armored
Double-Jacket Optical Fiber Cables (contd.)
Ordering Information - Multi-Unit Cables
FF: Fiber Type
Cable
Max. Load N
Fiber per
Subunit
Weight
Description
OD
Packaging
P/N
Short
Long
Subunit
Count
Kg/Km
mm
Term
Term
18-Fiber FO Outdoor Steel Armored
6
3
17
290
1700
800
2000m Drum
23D FF CN018M-BK2N
Tight-Buffer DJ Cable
24-Fiber FO Outdoor Steel Armored
6
4
18
315
1700
800
2000m Drum
23D FF CN024M-BK2N
Tight-Buffer DJ Cable
36-Fiber FO Outdoor Steel Armored
6
6
21
420
1700
800
2000m Drum
23D FF CN036M-BK2N
Tight-Buffer DJ Cable
48-Fiber FO Outdoor Steel Armored
12
4
21
420
1700
800
2000m Drum
23D FF CN048M-BK2N
Tight-Buffer DJ Cable
60-Fiber FO Outdoor Steel Armored
12
5
22
450
1700
800
2000m Drum
23D FF CN060M-BK2N
Tight-Buffer DJ Cable
72-Fiber FO Outdoor Steel Armored
12
6
24
540
1700
800
2000m Drum
23D FF CN072M-BK2N
Tight-Buffer DJ Cable
96-Fiber FO Outdoor Steel Armored
12
8
27
665
1700
800
2000m Drum
23D FF CN096M-BK2N
Tight-Buffer DJ Cable
144-Fiber FO Outdoor Steel Armored
12
12
33
940
1700
800
2000m Drum
23D FF CN144M-BK2N
Tight-Buffer DJ Cable
B.1.7.7a