AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 6A
S/FTP 100 Ohm Indoor Flexible LAN Cables
Description
4 pair S/FTP flexible cables
Frequency range
1-500 MHz
Conductor
26 AWG 7x0.16mm stranded
bare copper
Insulation
PO
Color code
ANSI/TIA-568-C.2
Individual shield
Aluminum foil
Overall shield
Tin-coated copper braid
Drain wire
None
Jacket
PVC or LS0H
Standard & EU Directives Conformance
• Category 6A work area cable according to IEC 61156-6
• Category 6A cord cable according to ANSI/TIA-568-C.2
• 500MHz work area cable according to EN 50288-11-1
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034 (LS0H cables)
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm 2 max.
Short term bend radius
8xOD mm
Long term bend radius
4xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
DC resistance
145 Ohm/Km max.
Capacitance
56 pF/m max. @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
80% nom.
Ordering Information
OD
Weight
Description
Packaging
P/N
mm
Kg/Km
4-Pair 26 AWG S/FTP CAT6A PVC IEC 60332-1 Flexible Cable Gray
6.2
42
500m Drum
12S6AVA004N-GY2K
4-Pair 26 AWG S/FTP CAT6A LS0H IEC 60332-1 Flexible Cable Gray
6.2
42
500m Drum
12S6AHA004N-GY2K
4-Pair 26 AWG S/FTP CAT6A PVC IEC 60332-1 Flexible Cable Gray
6.2
42
1000m Drum
12S6AVA004N-GY2L
4-Pair 26 AWG S/FTP CAT6A LS0H IEC 60332-1 Flexible Cable Gray
6.2
42
1000m Drum
12S6AHA004N-GY2L
A.5.2.2