AT&T Cabling Systems
FiberLine
AT&T FiberLine
Single Loose-Tube Dielectric FTTx Drop Optical Fiber Cables
Description
2-12 fibers single loose-tube dielectric FTTx drop FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
Single PBT jell-filled loose tube
Strength elements
Two rigid FRP rods
Water blocking
Swellable fillers
Cable jacket material
UV-resistant PE
Cable formation
Flat-oval
Fibers color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
30xOD mm
Long term bend radius
15xOD mm
Operating temperature
-30 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Ordering Information
FF: Fiber Type
Cable
Max. Load N
Weight
Description
OD
Short
Long
Packaging
P/N
Kg/Km
mm
Term
Term
2-Fiber FO Dielectric Single Loose-Tube FTTx Drop Cable
6.0x9.0
40.0
1350
400
2000m Drum
24P FF EN002N-BK2N
4-Fiber FO Dielectric Single Loose-Tube FTTx Drop Cable
6.0x9.0
40.0
1350
400
2000m Drum
24P FF EN004N-BK2N
6-Fiber FO Dielectric Single Loose-Tube FTTx Drop Cable
6.0x9.0
40.0
1350
400
2000m Drum
24P FF EN006N-BK2N
8-Fiber FO Dielectric Single Loose-Tube FTTx Drop Cable
6.0x9.0
40.0
1350
400
2000m Drum
24P FF EN008N-BK2N
10-Fiber FO Dielectric Single Loose-Tube FTTx Drop Cable
6.0x9.0
40.0
1350
400
2000m Drum
24P FF EN010N-BK2N
12-Fiber FO Dielectric Single Loose-Tube FTTx Drop Cable
6.0x9.0
40.0
1350
400
2000m Drum
24P FF EN012N-BK2N
B.1.8.2