AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor/Outdoor Tight-Buffer Non-Armored Optical Fiber LS0H Cables
Description
2-144 fibers indoor/outdoor tight-buffer non-armored FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
900µ tight flame retardant LS0H
coating
Strength elements
Served swellable aramid and glass
yarn
Central strength member
Dielectric, in multi-unit cables only
Sub-units jacket material
Flame retardant LS0H compound
Multi-unit water blocking
Swellable tapes
Cable jacket material
Flame retardant LS0H UV-resistant
compound
Fibers and sub-units color code TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame tests
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Ordering Information - Single Unit Cables
FF: Fiber Type
Cable
Max. Load N
Fiber
Weight
Description
OD
Packaging
P/N
Short
Long
Count
Kg/Km
mm
Term
Term
2-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
2
3.5
15
600
200
2000m Drum
23R FF HA002S-BK2N
4-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
4
5.0
22
600
200
2000m Drum
23R FF HA004S-BK2N
6-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
6
5.0
23
600
200
2000m Drum
23R FF HA006S-BK2N
8-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
8
5.5
27
600
200
2000m Drum
23R FF HA008S-BK2N
12-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
12
6.3
35
600
200
2000m Drum
23R FF HA012S-BK2N
16-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
16
7.0
45
1500
500
2000m Drum
23R FF HA016S-BK2N
18-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
18
7.5
51
1500
500
2000m Drum
23R FF HA018S-BK2N
24-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
24
8.5
60
1500
500
2000m Drum
23R FF HA024S-BK2N
Ordering Information - Multi-Unit Cables
FF: Fiber Type
Fiber
Cable
Max. Load N
Subunit
Weight
Description
per
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Subunit
mm
Term
Term
18-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
6
3
12
125
1500
500
2000m Drum
23R FF HA018M-BK2N
24-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
6
4
13
135
1500
500
2000m Drum
23R FF HA024M-BK2N
36-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
6
6
16
210
1500
500
2000m Drum
23R FF HA036M-BK2N
48-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
12
4
16
210
1500
500
2000m Drum
23R FF HA048M-BK2N
60-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
12
5
17
230
1500
500
2000m Drum
23R FF HA060M-BK2N
72-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
12
6
19
300
1500
500
2000m Drum
23R FF HA072M-BK2N
96-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
12
8
22
390
1500
500
2000m Drum
23R FF HA096M-BK2N
144-Fiber LS0H FO Indoor/Outdoor Tight-Buffer Cable
12
12
28
600
1500
500
2000m Drum
23R FF HA144M-BK2N
B.1.2.1