AT&T Cabling Systems
Outdoorline
AT&T Outdoorline LAN Copper Connectivity
Industrial Connection Boxes
Description
1-4 port stainless-steel IP67 industrial outdoor connection boxes
Jack compatibility
Shielded & unshielded RJ45 industrial
jacks
Category compatibility
CAT5e or CAT6
Mount type
Wall
Box color
White
Faceplate color
Metal
KSJ insertion method
Internal
Accessories
Cable glands, sealing inserts, screws
Gland cable OD limitation
11.0 mm max
Standard & EU Directives Conformance
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
• IEC 60259 IP67
• UL 1863 Communications-Circuit Accessories Safety
Mechanical & Electrical Properties
Material of construction - box
High-impact FR UV-resistant
plastic
Material of construction - cover
Stainless steel with rubber seal
Operating temperature
-25 to +70C at 5-95% RH
(Non condensing)
Storage temperature
-25 to +80C
Ordering Information
Box
Faceplate
Size
Description
Ports
Glands
Seals
Labeling
Packaging
P/N
Color
Color
mm
Industrial IP67 Outdoor
White
Metal
1
1
0
128x128x60
None
1/Bag 1/Box
16D00FV001B-MT51
Connection Box
Industrial IP67 Outdoor
White
Metal
2
2
1
128x128x60
None
1/Bag 1/Box
16D00FV002B-MT51
Connection Box
Industrial IP67 Outdoor
White
Metal
3
3
2
128x128x60
None
1/Bag 1/Box
16D00FV003B-MT51
Connection Box
Industrial IP67 Outdoor
White
Metal
4
4
3
128x128x60
None
1/Bag 1/Box
16D00FV004B-MT51
Connection Box
E.3.8