AT&T Cabling Systems
FiberLine
AT&T FiberLine Panels
Standard 19” Fiber Optic Panels
Description
1-288 fiber, 2-7U standard 19" fiber optic splicing/distribution panels
Connector type compatibility - Group A ST, SC, FC
Connector type compatibility - Group B LC, MTRJ, LSH (E-2000™)
Splicing with Group A & B connectors
Up to two 36 fiber splicing
in each cassette
Distribution with Group A connectors
Up to 24 fiber direct cable
termination in each U
Distribution with Group B connectors
Up to 48 fiber direct cable
termination in each U
Panel front
Up to 24 removable
modules
Panel access
Top and side
Front Cable Management
Tray for patch cord routing
and protection
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Steel, colored black
Front cover
Hinged transparent cover
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant materials
Port identification
Numbers and designated space
printed on the cover
Panel identification
Designated space at the panel front
Ordering Information - Panels
Fiber
Cassette
Module
Size
Description
Units
Capacity
Packaging
P/N
Capacity
Capacity
mm
A
B
Standard 2U Blank 19" Fiber Optic Panel
2U
36
72
2
6
83x483x356
1/Box
27S00NV072A-MT2U
Standard 3U Blank 19" Fiber Optic Panel
3U
72
144
4
12
132x483x356
1/Box
27S00NV144A-MT3U
Standard 7U Blank 19" Fiber Optic Panel
7U
144
288
8
24
293x483x356
1/Box
27S00NV288A-MT7U
Continued on page B.2.1.1a
B.2.1.1