AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 6
S/FTP 100 Ohm Horizontal Outdoor DJ LAN Cables
Description
4 pair S/FTP outdoor double-jacketed cables
Frequency range
1-250 MHz
Conductor
23 AWG Solid bare copper
Insulation
PO
Color code
Modified ANSI/TIA-568-C.2 (Solid colors)
Water blocking
None
Individual pair shield
Aluminum foil
Overall shield
Tin-coated copper braid
Drain wire
None
Inner jacket
PVC or LS0H
Outer jacket - Option A
1.8 mm UV resistant PVC compound for
outdoor use
Outer jacket - Option B
1.0 mm UV resistant MDPE for outdoor
use
Outer jacket color
Black
Standard & EU Directives Conformance
• Category 6 cable according to ANSI/TIA-568-C.2
• Category 6 cable according to IEC 61156-5
• 250 MHz cable according to EN 50288-5-1
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max.
Dynamic bend radius
8xOD mm min
Static bend radius
4xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
80 Ohm/Km max.
Capacitance
56 pF/m max. @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
78% nom.
Ordering Information
Inner
Outer
OD
Weight
Description
Jacket
Jacket
Packaging
P/N
mm
Kg/Km
Type
Type
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
PVC
PVC
10.7
123
500m drum
11S06BN004A-BK2K
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
PVC
PVC
10.7
123
1000m drum
11S06BN004A-BK2L
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
PVC
PE
9.1
76
500m drum
11S06EN004A-BK2K
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
PVC
PE
9.1
76
1000m drum
11S06EN004A-BK2L
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
LS0H
PVC
10.7
123
500m drum
11S06BN004B-BK2K
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
LS0H
PVC
10.7
123
1000m drum
11S06BN004B-BK2L
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
LS0H
PE
9.1
76
500m drum
11S06EN004B-BK2K
4-Pair 23 AWG S/FTP CAT6 Outdoor DJ Cable Black
LS0H
PE
9.1
76
1000m drum
11S06EN004B-BK2L
E.2.5