AT&T Cabling Systems
Outdoorline
AT&T Outdoorline
Outdoor Fiber-optic Splice Closures
Description
Outdoor dome-structure fiber-optic splice closures with
heat-shrink seals
Installation options
Aerial, duct, pole, wall
and direct-burial
Limitations
Not suitable for water immersion
Cable types compatibility
Round Loose-tube, tight-buffer or
ribbon FO cables
Structure
Dome type
Dome material of construction
Heavy duty, UV-resistant
high-impact material
Color
Black
Operating temperature
-40 to +65C at 5-95% RH
(Non condensing)
Installation temperature
0 to +50C
Standard & EU Directives Conformance
• EU Directive 2011/65/EU (RoHS-2)
• IEC 60259 IP68
Components
Protective dome (cover)
1
Splicing trays
Included
Support tray
1
Unit base
1
Bracket
1
Sealing gasket
1
Pressure valve
1
Grounding kit
1 set
Essential accessories
Included
Ordering Information
Size mm
Cable Ports
FO
Total
Splicing
Single
Max.
Description
Cable
Fiber
Tray
Tray
Packaging
P/N
Amount
Cable
Height
Diameter
Type
Capacity
Type
Capacity
& Type
Diameter
mm
Outdoor Fiber-optic
3 Round
16.0
Dome Splice Closure
435
190
Round
72
CA
12
1/Box
53S00KNG0A1-BK51
Type G0A1
1 Oval
25.0
Outdoor Fiber-optic
3 Round
16.0
Dome Splice Closure
435
190
Round
48-96
CB
24
1/Box
53S00KNG0A2-BK51
Type G0A2
1 Oval
25.0
Outdoor Fiber-optic
4 Round
20.0
Dome Splice Closure
495
220
Round
120
CA
12
1/Box
53S00KNG0D1-BK51
Type G0D1
1 Oval
35.0
Outdoor Fiber-optic
4 Round
20.0
Dome Splice Closure
495
220
Round
288
BG
48
1/Box
53S00KNG0D2-BK51
Type G0D2
1 Oval
35.0
Outdoor Fiber-optic
4 Round
20.0
Dome Splice Closure
495
220
Round
432
BI
72
1/Box
53S00KNG0D3-BK51
Type G0D3
1 Oval
35.0
Continued on page E.5.1a
E.5.1