AT&T Cabling Systems
RackLine
AT&T RackLine
Basic Power Distribution Units (PDU)
Description
Basic power distribution units for racks and cabinets
Nominal input voltage
250V AC single phase
Optional rated current
13A, 16A or 32A
Optional power plug types
IEC 60309, DIN 49441 or BS 1363
with 3m line cord
Output sockets
CEE 7/4 ("Schuko") or BS 1363
Power switch
Circuit breaker
Standard & EU Directives Conformance
• EN-55022 Class B (EMC)
• EU 2006/95/EC (LVD)
• EU 2011/65/EU (RoHS-2)
• IEC 60950 Para. 2.1 (Electrical safety)
Features and Properties
Mounting options
1U, 2U and Zero U rack mount
Material
Extruded aluminum chassis
Color
Black
Circuit breaker
16A with safety cover
Ordering Information
CEE 7/4
Plug
BS 1363
Circuit
Dimensions
Description
Schuko
Size
P/N
Type
Sockets
Breakers
mm
Sockets
16A 1U Basic PDU
DIN 49441
6
None
1x16A
1U
483x44x44
61416A1U06A-BK51
16A 2U Basic PDU
DIN 49441
9
None
1x16A
2U
483x89x44
61416A2U09A-BK51
13A 1U Basic PDU
BS 1363
None
6
On/Off
1.5U
483x67x44
61413A1U06A-BK51
32A Zero U Basic PDU
IEC 60309
18
None
2x16A
Zero U
1612x44x66
61432A0U18A-BK51
32A Zero U Basic PDU
IEC 60309
24
None
2x16A
Zero U
1612x44x66
61432A0U24A-BK51
D.6