AT&T Cabling Systems
CopperLine
AT&T CopperLine Outlets
UK Style Faceplates
Description
1-4 port UK Style faceplates
Jack compatibility
Shielded or unshielded RJ45
keystone jacks
Category compatibility
CAT5e CAT6 CAT6A
Mount type
Wall or ducts
Shuttered
Yes
Color
White (other colors available)
KSJ insertion method
Back loading
Standard & EU Directives Conformance
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Material of construction
High-impact flame retardant
materials
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Storage temperature
-20 to +80C
Ordering Information
Size
Description
Color
Ports
Labeling
Packaging
P/N
mm
UK Style Standard Back Box
White
N/A
87x87x38
None
1/Bag
16U00NV000A-WT61
UK Style Double Back Box
White
N/A
147x87x38
None
1/Bag
16U00NV000B-WT61
UK Style Faceplate with 50x50mm Opening
White
N/A
86x86x15
None
1/Bag
16U00NV000C-WT61
UK Style Faceplate with 100x50mm Opening
White
N/A
145x86x15
None
1/Bag
16U00NV000D-WT61
UK Style Single-Port Flat Half-Size Module
White
1
50x25
Station ID
1/Bag
16U00NV001A-WT61
UK Style Single-Port Angled Half-Size Module
White
1
50x25
Station ID
1/Bag
16U00NV001B-WT61
UK Style Blank Flat Full-Size Module
White
0
50x50
None
1/Bag
16U00NV000E-WT61
UK Style Blank Flat Half-Size Module
White
0
50x25
None
1/Bag
16U00NV000F-WT61
UK Style Blank Flat Quarter-Size Module
White
0
50x12.5
None
1/Bag
16U00NV000G-WT61
A.11.2