AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 7A
S/FTP 100 Ohm Horizontal Indoor LAN Cables
Description
4 & 8 pair S/FTP cables
Operation frequency range
1-1000 MHz
Testing frequency range
1-1200 MHz
Conductor
22 AWG Solid bare copper
Insulation
PO
Color code
Modified ANSI/TIA-568-C.2
(solid colors)
Individual pair shield
Aluminum foil
Overall shield
Tin-coated copper braid
Drain wire
None
Jacket
PVC or LS0H
Standard & EU Directives Conformance
• Category 7A cable according to IEC 61156-5
• 1000MHz cable according to EN 50288-11
• IEC 60332-1, IEC 60332-3-24 or IEC 60332-3-25 flame tests
• IEC 60754 & IEC 61034 (LS0H cables)
• EU Directive 2011/65/EU (RoHS-2)
• EU CPR 305/2011/EC B2ca s1 d0 classification upon request
Mechanical & Electrical Properties
Pulling force
50 N/mm 2 max.
Short term bend radius
8xOD mm
Long term bend radius
4xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
DC resistance
70 Ohm/Km max.
Capacitance
56 max. pF/m @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
78% nom.
Ordering Information
OD
Weight
Description
Packaging
P/N
mm
Kg/Km
4-Pair 22 AWG S/FTP CAT7A PVC IEC 60332-1 Cable Gray
7.2
55
500m drum
11S7AVA004A-GY2K
4-Pair 22 AWG S/FTP CAT7A LS0H IEC 60332-1 Cable Gray
7.2
55
500m drum
11S7AHA004A-GY2K
4-Pair 22 AWG S/FTP CAT7A PVC IEC 60332-1 Cable Gray
7.2
55
1000m drum
11S7AVA004A-GY2L
4-Pair 22 AWG S/FTP CAT7A LS0H IEC 60332-1 Cable Gray
7.2
55
1000m drum
11S7AHA004A-GY2L
2x(4-Pair 22 AWG S/FTP) CAT7A PVC IEC 60332-1 FIG-8 Cable Gray
7.2x14.4
110
500m drum
11S7AVA008B-GY2K
2x(4-Pair 22 AWG S/FTP) CAT7A LS0H IEC 60332-1 FIG-8 Cable Gray
7.2x14.4
110
500m drum
11S7AHA008B-GY2K
A.7.1.2