AT&T Cabling Systems
FiberLine
AT&T FiberLine Panels
Basic 19” Fiber Optic Panels
Description
1-48 fiber 1U low-cost fixed 19" fiber optic splicing/distribution
panels
Connector type compatibility - Group A ST, SC, FC, LC, MTRJ, LSH
(E-2000™)
Splicing
Up to two 24 fiber splicing
cassettes
Distribution
Up to 48 fiber direct cable
termination
Panel access
Top and front sliding tray
Back Cable Management
None
Front Cable Management
None
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
SPCC Steel, colored black
Front cover
None
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant materials
Port identification
Numbers and designated space
printed on the cover
Ordering Information
Compatible
Coupler
Fiber
Cassette
Size
Description
Packaging
P/N
Couplers
Capacity
Capacity
Capacity
mm
Basic 1U Blank 19” Fiber Optic Panel
ST Simplex
24
24
1
44.5x483x230
1/Box
27B00NV024A-BK1U
Basic 1U Blank 19” Fiber Optic Panel
SC Simplex
24
24
1
44.5x483x230
1/Box
27B00NV024H-BK1U
Basic 1U Blank 19” Fiber Optic Panel
SC Duplex
12
24
1
44.5x483x230
1/Box
27B00NV024J-BK1U
Basic 1U Blank 19” Fiber Optic Panel
SC Duplex
24
48
2
44.5x483x230
1/Box
27B00NV048J-BK1U
Basic 1U Blank 19” Fiber Optic Panel
FC Simplex
24
24
1
44.5x483x230
1/Box
27B00NV024E-BK1U
Basic 1U Blank 19” Fiber Optic Panel
LC Duplex
12
24
1
44.5x483x230
1/Box
27B00NV024Q-BK1U
Basic 1U Blank 19” Fiber Optic Panel
LC Duplex
24
48
2
44.5x483x230
1/Box
27B00NV048Q-BK1U
Basic 1U Blank 19” Fiber Optic Panel
MTRJ
12
24
1
44.5x483x230
1/Box
27B00NV024S-BK1U
Basic 1U Blank 19” Fiber Optic Panel
MTRJ
24
48
1
44.5x483x230
1/Box
27B00NV048S-BK1U
B.2.1.3