AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 6
U/FTP 100 Ohm Horizontal Indoor LAN Cables
Description
4 & 8 pair U/FTP cables
Frequency range
1-250 MHz
Conductor
23 AWG Solid bare copper
Insulation
PO
Color code
Modified ANSI/TIA-568-C.2
(solid colors)
Shield
Individual pair aluminum foil
Drain wire
Single tin-coated copper solid
wire
Jacket
PVC or LS0H
Standard & EU Directives Conformance
• Category 6 cable according to IEC 61156-5
• Category 6 cable according to ANSI/TIA-568-C.2
• 250MHz cable according to EN 50288-5-1
• IEC 60332-1, IEC 60332-3-24 or IEC 60332-3-25 flame tests
• IEC 60754 & IEC 61034 (LS0H cables)
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm 2 max.
Short term bend radius
8xOD mm
Long term bend radius
4xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
DC resistance
80 Ohm/Km max.
Capacitance
56 max. pF/m @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
78% nom.
Ordering Information
OD
Weight
Description
Packaging
P/N
mm
Kg/Km
4-Pair 23 AWG U/FTP CAT6 PVC IEC 60332-1 Cable Gray
7.0
48
500m drum
11F06VA004N-GY2K
4-Pair 23 AWG U/FTP CAT6 LS0H IEC 60332-1 Cable Gray
7.0
48
500m drum
11F06HA004N-GY2K
4-Pair 23 AWG U/FTP CAT6 PVC IEC 60332-1 Cable Gray
7.0
48
1000m drum
11F06VA004N-GY2L
4-Pair 23 AWG U/FTP CAT6 LS0H IEC 60332-1 Cable Gray
7.0
48
1000m drum
11F06HA004N-GY2L
2x(4-Pair 23 AWG U/FTP) CAT6 PVC IEC 60332-1 FIG-8 Cable Gray
7.0x14.0
96
500m drum
11F06VA008F-GY2K
2x(4-Pair 23 AWG U/FTP) CAT6 LS0H IEC 60332-1 FIG-8 Cable Gray
7.0x14.0
96
500m drum
11F06HA008F-GY2K
A.4.1.3