AT&T Cabling Systems
CopperLine
AT&T CopperLine Outlets
US Style Faceplates
Description
1-6 port US Style faceplates
Jack compatibility
Shielded or unshielded RJ45
keystone jacks
Category compatibility
CAT5e CAT6 CAT6A
Mount type
Wall or ducts
Shuttered
Optional
Color
White (other colors available)
KSJ insertion method
Back loading
Standard & EU Directives Conformance
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Material of construction
High-impact flame retardant
materials
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Storage temperature
-20 to +80C
Ordering Information
Size
Description
Color
Ports
Labeling
Packaging
P/N
mm
US Style Back Box
White
N/A
115x72x38
None
1/Bag
16A00NV000A-WT61
US Style Faceplate, Single Port, No Shutter
White
1
113x70
Station ID
1/Bag
16A00NV001A-WT61
US Style Faceplate, Two Ports, No Shutter
White
2
113x70
Station ID
1/Bag
16A00NV002A-WT61
US Style Faceplate, Three Ports, No Shutter
White
3
113x70
Station ID
1/Bag
16A00NV003A-WT61
US Style Faceplate, Four Ports, No Shutter
White
4
113x70
Station ID
1/Bag
16A00NV004A-WT61
US Style Faceplate, Six Ports, No Shutter
White
6
113x70
Station ID
1/Bag
16A00NV006A-WT61
US Style Faceplate, Single Port, with Shutter
White
1
113x70
None
1/Bag
16A00NV001B-WT61
US Style Faceplate, Two Ports, with Shutter
White
2
113x70
None
1/Bag
16A00NV002B-WT61
US Style Faceplate, Four Ports, with Shutter
White
4
113x70
None
1/Bag
16A00NV004B-WT61
A.11.4