AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 6
U/UTP 100 Ohm Indoor Flexible LAN Cables
Description
4 pair U/UTP flexible cables
Frequency range
1-250 MHz
Conductor
24 AWG 7x0.20mm stranded
bare copper
Insulation
PO
Color code
ANSI/TIA-568-C.2
Shield
None
Jacket
PVC or LS0H
Standard & EU Directives Conformance
• Category 6 work area cable according to IEC 61156-6
• Category 6 cord cable according to ANSI/TIA-568-C.2
• 250MHz work area cable according to EN 50288-6-2
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034 (LS0H cables)
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm 2 max.
Short term bend radius
8xOD mm
Long term bend radius
4xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max.
Capacitance
56 pF/m max. @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
69% nom.
Ordering Information
OD
Weight
Description
Packaging
P/N
mm
Kg/Km
4-Pair 24 AWG U/UTP CAT6 PVC IEC 60332-1 Flexible Cable Gray
6.0
40
500m Drum
12U06VA004N-GY2K
4-Pair 24 AWG U/UTP CAT6 LS0H IEC 60332-1 Flexible Cable Gray
6.0
40
500m Drum
12U06HA004N-GY2K
4-Pair 24 AWG U/UTP CAT6 PVC IEC 60332-1 Flexible Cable Gray
6.0
40
1000m Drum
12U06VA004N-GY2L
4-Pair 24 AWG U/UTP CAT6 LS0H IEC 60332-1 Flexible Cable Gray
6.0
40
1000m Drum
12U06HA004N-GY2L
A.4.2.1