AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MPO Plug & Play
High-Density MPO Fixed Fiber Optic Panels
Description
72-144 fiber 1U 19" high-density MPO fixed fiber optic panels
Panel front
72, 96 or 144 LC/UPC ports
Panel back
Six, eight or twelve 12-fiber MPO
couplers
Fiber type compatibility
OM1, OM2, OM3, OM4 & OS2
Back Cable Management
Removable tray with strain relief
Front Cable Management
Removable tray for patch cord
routing and protection
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Steel, colored black
Front cover
None
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant materials
Port identification
Numbers
Ordering Information
Fiber
Fiber
MPO
Size
Description
Polarity
Packaging
P/N
Type
Capacity
Couplers
mm
High-Density MPO to LC/UPC
OM1
72
6
Straight
44.5x483x336
1/Box
27PM1HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM1
72
6
Flipped
44.5x483x336
1/Box
27EM1HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM2
72
6
Straight
44.5x483x336
1/Box
27PM2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM2
72
6
Flipped
44.5x483x336
1/Box
27EM2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3
72
6
Straight
44.5x483x336
1/Box
27PM3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3
72
6
Flipped
44.5x483x336
1/Box
27EM3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3 BI
72
6
Straight
44.5x483x336
1/Box
27PC3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3 BI
72
6
Flipped
44.5x483x336
1/Box
27EC3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4
72
6
Straight
44.5x483x336
1/Box
27PM4HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4
72
6
Flipped
44.5x483x336
1/Box
27EM4HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4 BI
72
6
Straight
44.5x483x336
1/Box
27PC4HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4 BI
72
6
Flipped
44.5x483x336
1/Box
27EC4HV072P-BK1U
Fixed Fiber Optic Panel
Continued on page B.5.2.3a
BI = Bend-Insensitive
C.5.2.3