AT&T Cabling Systems
Outdoorline
AT&T Outdoorline LAN Copper Connectivity
Industrial Faceplates
Description
1-4 port stainless-steel IP67 industrial outdoor faceplates
Jack compatibility
Shielded & Unshielded RJ45
Industrial Jacks
Category compatibility
CAT5e or CAT6
Mount type
Wall or duct
Color
Metal
KSJ insertion method
Back loading
Accessories
2 Screws
Standard & EU Directives Conformance
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
• IEC 60259 IP67
• UL 1863 Communications-Circuit Accessories Safety
Mechanical & Electrical Properties
Material of construction
Stainless steel with rubber seal
Operating temperature
-25 to +70C at 5-95% RH
(Non condensing)
Storage temperature
-25 to +80C
Ordering Information
Description
Color
Ports
Size mm
Labeling
Packaging
P/N
Industrial IP67 Stainless Steel faceplate
Metal
1
70x115x4.4
None
1/Bag
16D00FV001A-MT61
Industrial IP67 Stainless Steel faceplate
Metal
2
70x115x4.4
None
1/Bag
16D00FV002A-MT61
Industrial IP67 Stainless Steel faceplate
Metal
4
116.5x11x4.4
None
1/Bag
16D00FV004A-MT61
E.3.7