AT&T Cabling Systems
FiberLine
AT&T FiberLine
Microduct Dry-Core FTTx Optical Fiber Cables
Description
2-72 fibers outdoor all-dielectric microduct dry-core single-jacket
non-armored FTTx FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
PBT jell-filled loose tubes
Central strength member
Rigid all-dielectric FRP
Water blocking elements
Swellable yarn and tapes
Cable jacket material
UV-resistant PE
Fibers and tubes color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
25xOD mm
Long term bend radius
15xOD mm
Operating temperature
-30 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Default fiber count per tube
Indicated (other options available)
Ordering Information
FF: Fiber Type
Fibers
Cable
Max. Load N
Tube
Weight
Description
per
Fillers
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Tube
mm
Term
Term
2-Fiber FO Microduct FTTx
2000m
2
1
5
6.0
38.0
700
420
25F FF EN002N-BK2N
All-Dielectric Dry-Core Cable
Drum
4-Fiber FO Microduct FTTx
2000m
4
1
5
6.0
38.0
700
420
25F FF EN004N-BK2N
All-Dielectric Dry-Core Cable
Drum
6-Fiber FO Microduct FTTx
2000m
6
1
5
6.0
38.0
700
420
25F FF EN006N-BK2N
All-Dielectric Dry-Core Cable
Drum
8-Fiber FO Microduct FTTx
2000m
8
1
5
6.0
38.0
700
420
25F FF EN008N-BK2N
All-Dielectric Dry-Core Cable
Drum
12-Fiber FO Microduct FTTx
2000m
12
1
5
6.0
38.0
700
420
25F FF EN012N-BK2N
All-Dielectric Dry-Core Cable
Drum
24-Fiber FO Microduct FTTx
2000m
12
2
4
6.0
38.0
700
420
25F FF EN024N-BK2N
All-Dielectric Dry-Core Cable
Drum
36-Fiber FO Microduct FTTx
2000m
12
3
3
6.0
38.0
700
420
25F FF EN036N-BK2N
All-Dielectric Dry-Core Cable
Drum
48-Fiber FO Microduct FTTx
2000m
12
4
2
6.0
38.0
700
420
25F FF EN048N-BK2N
All-Dielectric Dry-Core Cable
Drum
72-Fiber FO Microduct FTTx
2000m
12
6
0
6.0
38.0
700
420
25F FF EN072N-BK2N
All-Dielectric Dry-Core Cable
Drum
B.1.8.1