AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic Panels
Wall-Mount Indoor Fiber Optic Panels
Description
12 or 24 fiber indoor wall-mount panels
Connector type compatibility
ST, SC, FC, LC, MTRJ, LSH (E-2000™)
Splicing
One or two 12 fiber splicing
cassettes
Distribution
12 or 24 fiber direct cable
termination
Panel front
Two or four removable pre-loaded
modules
Panel access
Front
Doors
Two individually locked doors
Locking method
Mechanical key
Mounting orientation
Horizontal or vertical
Mounting method
Screws (not included)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Galvanized steel colored gray
Front cover
None
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant
materials
Port identification
Numbers
Panel identification
Designated space inside the panel
Ordering Information - Panels
Fiber
Cassette
Module
Size
Description
Packaging
P/N
Capacity
Capacity
Capacity
mm
12 Fiber Blank Wall-Mount Fiber Optic Panel
12
1
2
91x285x330
1/Box
27W00NV012N-GY51
24 Fiber Blank Wall-Mount Fiber Optic Panel
24
2
4
91x383x355
1/Box
27W00NV024N-GY51
Continued on page B.5.3.2a
C.5.3.2