AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic SC Connectors
Description
Fiber Optic Connectors Type SC
Durability
0.2dB max. change after 1000 mating cycles
Temperature range
-20 to +60C
Typical Insertion loss
<0.2dB
Connector Ferrule type
Ceramic
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• EU Directive 2011/65/EU (RoHS-2)
Notes:
a. Each product has a full-length P/N that can be used as ordering information.
b. Each connector has a single letter code that can be used to build fiber-optic cords and pigtails part-numbers.
c. The default colors are indicated in this page. Other options available.
d. Each bag contains one connector and two colored boots: 0.9mm & 3.0mm.
Ordering Information - Connectors
Compatible
Body
Type
Formation
Boot Color
Code
Packaging
P/N
Fiber
Color
SC/UPC Connector
Multimode
Single
Beige
Beige
H
1/Bag 120/Box
29CM1NV001H-BG61
SC/UPC Connector
Singlemode
Single
Blue
Blue
J
1/Bag 120/Box
29CS1NV001J-PB61
SC/APC Connector
Singlemode
Single
Green
Green
K
1/Bag 120/Box
29CS1NV001K-GN61
SC/UPC Connector
Multimode
Double
Beige
Red & Black
H
1/Bag 120/Box
29CM1NV002H-BG61
SC/UPC Connector
Singlemode
Double
Beige
Blue
J
1/Bag 120/Box
29CS1NV002J-PB61
SC/APC Connector
Singlemode
Double
Green
Green
K
1/Bag 120/Box
29CS1NV002K-GN61
Ordering Information - Clips
Type
Color
Packaging
P/N
Duplex Clip for SC/UPC Multimode Connector
Beige
120/Bag
531M1NV002H-BG6Y
Duplex Clip for SC/UPC Singlemode Connector
Blue
120/Bag
531S1NV002J-PB6Y
Duplex Clip for SC/APC Singlemode Connector
Green
120/Bag
531S1NV002K-GN6Y
B.4.1.3