AT&T Cabling Systems
CenterLine
AT&T CenterLine
DC Enclosures & Rack Cooling Containment Systems
Description
Data center cooling containment systems for hot or cold corridors
Top cover construction material
Steel framed reinforced
polycarbonate
Containment doors construction material Steel and tempered glass
Containment doors design
Double sliding doors with
look-through window
Containment doors locking options
Mechanical or electronic
Color
Black RAL 9005
Custom-made accessories
Air blocking material
Height adjustment panels
for lighting devices
Standard & EU Directives Conformance
• Mechanical structure conforming to EN 61587-1
• Corrosion resistance (salt spray) acc. to ISO 9227 & ASTM B117
• EU Directive 2011/65/EU (RoHS-2)
Optional Dimensions
Containment top cover width options
600, 800, 900
or 1100 mm
Cold corridor double door dimensions
42U x 1200 mm
or 47U x 1200 mm
Hot corridor single door dimensions
42U x 800 mm
or 47U x 800 mm
Ordering Information - Top Cover
Dimensions
Description
Color
P/N
mm
Hot Corridor Containment Top Cover
600x800
Black
42106800NAN-BK51
Hot Corridor Containment Top Cover
800x800
Black
42108800NAN-BK51
Hot Corridor Containment Top Cover
900x800
Black
42109800NAN-BK51
Hot Corridor Containment Top Cover
1100x800
Black
42111800NAN-BK51
Cold Corridor Containment Top Cover
600x1200
Black
42206120NAN-BK51
Cold Corridor Containment Top Cover
800x1200
Black
42208120NAN-BK51
Cold Corridor Containment Top Cover
900x1200
Black
42209120NAN-BK51
Cold Corridor Containment Top Cover
1100x1200
Black
42211120NAN-BK51
Ordering Information - Doors
Dimensions
Description
Size
Color
P/N
mm
Hot Corridor Containment Door System
42U
2028x800
Black
42342U08NAN-BK51
Hot Corridor Containment Door System
47U
2250x800
Black
42347U08NAN-BK51
Cold Corridor Containment Door System
42U
2028x1200
Black
42442U12NAN-BK51
Cold Corridor Containment Door System
47U
2250x1200
Black
42447U12NAN-BK51
C.1.4