AT&T Cabling Systems
CopperLine
AT&T CopperLine Panels
Unshielded Snap-in Blank Patch Panels for Straight Jacks
Description
24 & 48 port unshielded blank 19” panels
KSJ type compatibility
Unshielded 180° straight
RJ45 jacks
Category compatibility
CAT5e CAT6 CAT6A
KSJ insertion method
Back loading
Formation
24 ports in one row
Front cable organizer
Removable modular rings
Back cable organizer
Folding frame with snap-in
cable grips
Shield
None
Standard & EU Directives Conformance
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Galvanized corrosion resistant
steel
Paint
Powder paint finish
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Storage temperature
-20 to +80C
Plastic parts
High-impact flame retardant
materials
Port identification
Labels with transparent plastic
cover
Panel identification
Designated space at the panel
front
Ordering Information
Size
Description
Color
Units
Packaging
P/N
mm
24 Port Unshielded 19’’ Snap-in Blank Patch Panel (Straight Jacks)
Steel-Blue
1U
44.4x483
1/Box
13U00NV024A-SB1U
48 Port Unshielded 19’’ Snap-in Blank Patch Panel (Straight Jacks)
Steel-Blue
2U
89.0x483
1/Box
13U00NV048A-SB2U
A.10.1.1