AT&T Cabling Systems
FiberLine
AT&T FiberLine Panels
High-Density MTP Cassette Fiber Optic Panel
Description
1-120 fiber 1U 19" high-density MTP cassette fiber optic panel
Cassette front
12 or 24 LC/UPC ports
Cassette back options
One or two 12-fiber MTP couplers
Fiber type compatibility
OM1, OM2, OM3, OM4 & OS2
Panel front
Up to five removable pre-loaded
cassettes
Panel access
Top and front slide rail
Back Cable Management
Removable tray with strain relief
Front Cable Management
Tray with rings for patch cord
routing and protection
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Steel, colored black
Front cover
None
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant
materials
Port identification
Numbers
Ordering Information - Panel
Fiber
Cassette
Size
Description
Units
Packaging
P/N
Capacity
Capacity
mm
High-Density Blank MTP Cassette Fiber Optic Panel
1U
120
5
44.5x483x501
1/Box
27D00NV120A-BK1U
Continued on page B.2.2.2a
B.2.2.2