AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 6
Shielded RJ45 Plugs
Description
8P8C shielded RJ45 plugs
Frequency range
1-250 MHz
Compatible conductors
24-26 AWG Solid or stranded
Contacts
50µ-Inch Gold plating over
nickel plated copper alloy
Shield
Corrosion resistant metal casing
Housing
FR Polycarbonate
Standard & EU Directives Conformance
• 250MHz shielded connectors according to IEC 60603-7-5
• 250MHz shielded connectors according to EN 60603-7-5
• Category 6 connecting hardware according to
ANSI/TIA-568-C.2
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Ampacity
1.5 A max.
Cable form compatibility
Flat or round
Insertion/withdrawal
750 cycles Level A durability
Cable re-termination
0 terminations
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Contact resistance
20 mOhm max.
DC resistance
0.1 Ohm max.
Voltage rating
75 Vdc max.
Insulation resistance
500 MegaOhm min. @500 Vdc
Ordering Information
Description
Color
Conductor
Packaging
P/N
8P8C RJ45 Shielded CAT6 Plug
Transparent
Solid
100/Box
15S06NV008A-TP5C
8P8C RJ45 Shielded CAT6 Plug
Transparent
Stranded
100/Box
15S06NV008B-TP5C
8P8C RJ45 Shielded CAT6 Plug
Transparent
Solid & Stranded
100/Box
15S06NV008C-TP5C
A.4.3.2