AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 6
Unshielded RJ45 Punch-Down Keystone Jacks
Description
8P8C unshielded RJ45 punch-down keystone jacks
Frequency range
1-250 MHz
Compatible conductors
22-26 AWG Solid or stranded
Pin-pair assignment
T568A & T568B (Universal)
Contacts
50µ-Inch Gold plating
Shield
None
Housing
High impact FR compound
Standard color
White/Blue
(other colors available)
Standard & EU Directives Conformance
• 250MHz unshielded connectors according to IEC 60603-7-4
• 250MHz unshielded connectors according to EN 60603-7-4
• Category 6 connecting hardware according to
ANSI/TIA-568-C.2
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Orientation
180º
Termination blocks
110 IDC
Insertion/withdrawal
750 cycles
Cable re-termination
20 terminations
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Ampacity
1.5 A max.
Contact resistance
20 mOhm max.
DC resistance
0.1 Ohm max.
Voltage rating
75 Vdc max.
Insulation resistance
500 MegaOhm min. @500 Vdc
Recommended punch-down tool AT&T MultiPunch 4-pair
hand-tool
Straight jacks are compatible with 24-port & 48-port 1U panels
Angled jacks are compatible only with 24-port 2-row 1U panels
Ordering Information
Description
Color
Form
Packaging
P/N
8P8C RJ45 Unshielded CAT6 PD 180º Keystone Jack
White/Blue
Straight
1/Bag 96/Box
15A06NV008A-WB61
8P8C RJ45 Unshielded CAT6 PD 180º Keystone Jack
White/Blue
Angled
1/Bag 60/Box
15A06NV008B-WB61
A.4.3.3