AT&T Cabling Systems
CopperLine
AT&T CopperLine Outlets
Surface Mount Boxes
Description
1-4 port surface mount boxes
Jack compatibility
Shielded or unshielded RJ45
keystone jacks
Category compatibility
CAT5e CAT6 CAT6A
Mount type
Wall or ducts
Shuttered
Yes
Color
White (other colors available)
KSJ insertion method
Back loading (inside the box)
Standard & EU Directives Conformance
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Material of construction
High-impact flame retardant
materials
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Storage temperature
-20 to +80C
Ordering Information
Size
Description
Color
Ports
Labeling
Packaging
P/N
mm
Single Port Surface Mount Box
White
1
46x65x30.5
Station ID
1/Bag
16S00NV001A-WT61
Two Port Surface Mount Box
White
2
68x65x30.5
Station ID
1/Bag
16S00NV002A-WT61
Four Port Surface Mount Box
White
4
118x85.2x30.5
Station ID
1/Bag
16S00NV004A-WT61
A.11.5