AT&T Cabling Systems
CopperLine
AT&T CopperLine Accessories
Duct Type Cable Management Solutions
Description
Rack-mount duct-type 19" horizontal cable managers
Construction material
UV stabilized ABS
Position
Front or rear cable support
Cover
Included, removable
Color
Black
Size options
1U or 2U
Depth options
Available
Standard & EU Directives Conformance
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Construction
Solid and durable ABS mold
Cable retainers
Available in most types
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Ordering Information
Height
Width
Depth
Description
Retainers Units
Packaging
P/N
mm mm mm
Rack-Mount Duct-Type 19” Horizontal Cable Manager
None
1U
44.45
482.6
75.27
1/Box
521NANN075A-BK1U
Rack-Mount Duct-Type 19” Horizontal Cable Manager
Available
1U
44.3
482
162.83
1/Box
521NANN162B-BK1U
Rack-Mount Duct-Type 19” Horizontal Cable Manager
Available
2U
88.8
484.84
107.03
1/Box
521NANN107B-BK2U
Rack-Mount Duct-Type 19” Horizontal Cable Manager
Available
2U
88.8
484.74
171.62
1/Box
521NANN171B-BK2U
AT&T CopperLine Accessories
Ring Type Cable Management Solutions
Description
Rack-mount ring-type 19" horizontal cable managers
Construction material
UV stabilized ABS
Position
Front or rear cable support
Cover
Included, removable
Color
Black
Size options
1U
Depth options
Single
Standard & EU Directives Conformance
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Construction
Solid and durable ABS mold
Cable retainers
None
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Ordering Information
Description
Height
Width
Depth
Description
Retainers
Units
Packaging
P/N
mm
mm
mm
Height
Width
Depth
Description
Retainers
Units
Packaging
P/N
mm
mm
mm
Rack-Mount Ring-Type 19" Horizontal Cable Manager
None
1U
44.45
482.60
65.00
1/Box
521NANN065C-BK1U
A.12.2.1 - A.12.2.2