AT&T Cabling Systems
FiberLine
AT&T FiberLine Outlets
Fiber Optic Multimedia Boxes
Description
1-12 fiber multimedia boxes with fiber management
Connector type compatibility
ST, SC, LC and MTRJ
Type
Wall mount
Splicing and distribution options
1-12 fiber splicing
or cable distribution
Access method
Top and back
Standard & EU Directives Conformance
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Material of construction High-impact flame retardant materials
Operating temperature
0 to +60C at 5-85% RH (non condensing)
Storage temperature
-20 to +60C
Box identification
Label with transparent cover
Color
White RAL 1013
(other colors available)
Ordering Information - Multimedia Box
Fiber
Size
Description
Ports
Color
Packaging
P/N
Capacity
mm
12-Port Multimedia Box with Cable Management
12
1-24
205x171x57
White
1/Bag
53M2016012N-WT51
Ordering Information - Multimedia Box Inserts
Fiber
Size
Type
Adapter
Type
Color
Packaging
P/N
Capacity
mm
Inset Assembly for Multimedia Box
ST
Simplex
2
50x25x12
White
1/Bag
53MASNA002N-WT61
Inset Assembly for Multimedia Box
SC
Duplex
2
50x25x12
White
1/Bag
53MHDNA002N-WT61
Inset Assembly for Multimedia Box
LC
Quad
4
50x25x12
White
1/Bag
53MPQNA004N-WT61
Inset Assembly for Multimedia Box
LC
Duplex
2
50x25x12
White
1/Bag
53MPDNA002N-WT61
Inset Assembly for Multimedia Box
MTRJ
One Duplex
2
50x25x12
White
1/Bag
53MSSNA002N-WT61
Inset Assembly for Multimedia Box
MTRJ
Two Duplex
4
50x25x12
White
1/Bag
53MSDNA004N-WT61
Blank Inset for Multimedia Box
-
-
-
50x25x12
White
1/Bag
53M00NA000N-WT61
B.5.2