AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 6 LAN Copper Connectivity
Shielded & Unshielded RJ45 Industrial Plugs
Description
8P8C shielded & unshielded RJ45 IP67 industrial plugs
Frequency range
1-250 MHz
Compatible conductors
24-26 AWG Solid or stranded
Contacts
Gold plating over nickel plated
copper alloy
Shield (if present)
Corrosion resistant metal casing
Housing
FR Polycarbonate
Protective covers
FR UV-resistant heavy-duty
plastic material
Standard & EU Directives Conformance
• 250MHz connectors according to IEC 60603-7-4&5
• 2500MHz connectors according to EN 60603-7-4&5
• Category 6 connecting hardware acc. to ANSI/TIA-568-C.2
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
• IEC 60259 IP67
• UL 1863 Communications-Circuit Accessories Safety
Mechanical & Electrical Properties
Ampacity
1.5 A max.
Cable form compatibility
Flat or round
Insertion/withdrawal
750 cycles Level A durability
Cable re-termination
0 terminations
Operating temperature
-25 to +70C at 5-93% RH
(Non condensing)
Contact resistance
20 mOhm max.
DC resistance
0.1 Ohm max.
Voltage rating
75 Vdc max.
Insulation resistance
500 MegaOhm min. @500 Vdc
Ordering Information
Cover
Description
Plug Color
Conductor
Packaging
P/N
Color
8P8C RJ45 Unshielded CAT6 IP67 Industrial Plug
Transparent
Black
Solid
1/Bag
15U06FV008A-BK61
8P8C RJ45 Unshielded CAT6 IP67 Industrial Plug
Transparent
Black
Stranded
1/Bag
15U06FV008B-BK61
8P8C RJ45 Unshielded CAT6 IP67 Industrial Plug
Transparent
Black
Solid & Stranded
1/Bag
15U06FV008C-BK61
8P8C RJ45 Shielded CAT6 IP67 Industrial Plug
Transparent
Black
Solid
1/Bag
15S06FV008A-BK61
8P8C RJ45 Shielded CAT6 IP67 Industrial Plug
Transparent
Black
Stranded
1/Bag
15S06FV008B-BK61
8P8C RJ45 Shielded CAT6 IP67 Industrial Plug
Transparent
Black
Solid & Stranded
1/Bag
15S06FV008C-BK61
E.3.2