AT&T Cabling Systems
FiberLine
AT&T FiberLine Panels
High-Density MTP Fixed Fiber Optic Panel
Description
72-144 fiber 1U 19" high-density MTP fixed fiber optic panel
Panel front
72, 96 or 144 LC/UPC ports
Panel back
Six, eight or twelve 12-fiber MTP
couplers
Fiber type compatibility
OM1, OM2, OM3, OM4 & OS2
Back Cable Management
Removable tray with strain relief
Front Cable Management
Removable tray for patch cord
routing and protection
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Frame
Steel, colored black
Front cover
None
Operating temperature
-10 to +60C at 5-85% RH
(non condensing)
Storage temperature
-40 to +70C
Plastic parts
High-impact flame retardant
materials
Port identification
Numbers
Ordering Information
Fiber
Fiber
MTP
Size
Description
Polarity
Packaging
P/N
Type
Capacity
Couplers
mm
High-Density MTP to LC/UPC
OM1
72
6
Straight
44.5x483x336
1/Box
27FM1HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM1
72
6
Flipped
44.5x483x336
1/Box
27LM1HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM2
72
6
Straight
44.5x483x336
1/Box
27FM2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM2
72
6
Flipped
44.5x483x336
1/Box
27LM2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM3
72
6
Straight
44.5x483x336
1/Box
27FM3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM3
72
6
Flipped
44.5x483x336
1/Box
27LM3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM3 BI
72
6
Straight
44.5x483x336
1/Box
27FC3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM3 BI
72
6
Flipped
44.5x483x336
1/Box
27LC3HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM4
72
6
Straight
44.5x483x336
1/Box
27FM4HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM4
72
6
Flipped
44.5x483x336
1/Box
27LM4HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM4 BI
72
6
Straight
44.5x483x336
1/Box
27FC4HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MTP to LC/UPC
OM4 BI
72
6
Flipped
44.5x483x336
1/Box
27LC4HV072P-BK1U
Fixed Fiber Optic Panel
Continued on page B.2.2.3a
BI = Bend-Insensitive
B.2.2.3